| HOME / 정보공유 / AIX 명령어 모음

atmstat
atmstat atmstat 명령 목적 비동기 전송 모드 어댑터 통계를 표시합니다. 구문
atmstat [ -d -r ] Device_Name
설명
atmstat 명령은 비동기 전송 모드(ATM) 어댑터 통계를 표시합니다. 사용자는 장치 일반 통계와 함께 장치 고유 통계가 표시되도록 옵션으로 지정할 수 있습니다. 플래그가 지정되지 않으면, 장치 일반 통계만 표시됩니다. atmstat 명령의 실행에 따른 통계에 대한 보다 자세한 정보를 원하면 AIX 5L 버전 5.1 시스템 사용자 안내서: 통신 및 네트워크의 ATM 어댑터 통계를 보십시오.
유효하지 않은 Device_Name을 지정한 경우, atmstat 명령은 장치로 연결할 수 없음을 알리는 오류 메세지를 표시합니다.
플래그
-d 세부 통계를 표시합니다.
-r 모든 통계를 초기값으로 재설정합니다. 이 플래그는 특권 사용자만이 발행할 수 있습니다.
매개변수
Device_Name ATM 장치의 이름, 예를 들면, atm0.
예제
atm0에 대한 어댑터의 일반 통계를 표시하려면, 다음과 같이 입력하십시오.
atmstat atm0
이 명령은 마이크로채널 기계에 다음과 같은 출력을 생성합니다.
ATM STATISTICS (atm0) :
Device Type: Turboways 155 MCA ATM Adapter
Hardware Address: 08:00:5a:99:88:d5
Elapsed Time: 2 days 23 hours 38 minutes 18 seconds
Transmit Statistics: Receive Statistics:
-------------------- -------------------
Packets: 50573 Packets: 0
Bytes: 2225182 Bytes: 0
Interrupts: 0 Interrupts: 12904
Transmit Errors: 0 Receive Errors: 0
Packets Dropped: 0 Packets Dropped: 0
Bad Packets: 0
Max Packets on S/W Transmit Queue: 0
S/W Transmit Queue Overflow: 0
Current S/W+H/W Transmit Queue Length: 0
Cells Transmitted: 50573 Cells Received: 0
Out of Xmit Buffers: 0 Out of Rcv Buffers: 0
Current HW Transmit Queue Length: 0 CRC Errors: 0
Current SW Transmit Queue Length: 0 Packets Too Long: 0
Incomplete Packets: 0
Cells Dropped: 0
General Statistics:
-------------------
No mbuf Errors: 0
Adapter Loss of Signals: 0
Adapter Reset Count: 0
Driver Flags: Up Running Simplex
64BitSupport
Virtual Connections in use: 2
Max Virtual Connections in use: 2
Virtual Connections Overflow: 0
SVC UNI Version: auto_detect
Turboways ATM Adapter Specific Statistics:
---------------------------------------------------
Packets Dropped - No small DMA buffer: 0
Packets Dropped - No medium DMA buffer: 0
Packets Dropped - No large DMA buffer: 0
Receive Aborted - No Adapter Receive Buffer: 0
Transmit Attempted - No small DMA buffer: 0
Transmit Attempted - No medium DMA buffer: 0
Transmit Attempted - No large DMA buffer: 0
Transmit Attempted - No MTB DMA buffer: 0
Transmit Attempted - No Adapter Transmit Buffer: 0
Max Hardware transmit queue length: 12
Small Mbuf in Use: 0
Medium Mbuf in Use: 0
Large Mbuf in Use: 64
Huge Mbuf in Use: 0
MTB Mbuf in Use: 0
Max Small Mbuf in Use: 0
Max Medium Mbuf in Use: 0
Max Large Mbuf in Use: 64
Max Huge Mbuf in Use: 0
MTB Mbuf in Use: 0
Small Mbuf overflow: 0
Medium Mbuf overflow: 0
Large Mbuf overflow: 0
Huge Mbuf overflow: 0
MTB Mbuf overflow: 0
PCI 기계에 다음과 같은 출력을 생성합니다.
-------------------- -------------------
Packets: 299 Packets: 294
Bytes: 9727 Bytes: 10123
Interrupts: 0 Interrupts: 297
Transmit Errors: 0 Receive Errors: 0
Packets Dropped: 0 Packets Dropped: 0
Bad Packets: 0
Max Packets on S/W Transmit Queue: 0
S/W Transmit Queue Overflow: 0
Current S/W+H/W Transmit Queue Length: 2
Cells Transmitted: 450 Cells Received: 457
Out of Xmit Buffers: 0 Out of Rcv Buffers: 0
Current HW Transmit Queue Length: 2 CRC Errors: 0
Current SW Transmit Queue Length: 0 Packets Too Long: 0
Incomplete Packets: 0
Cells Dropped: 5
General Statistics:
-------------------
No mbuf Errors: 0
Adapter Loss of Signals: 0
Adapter Reset Count: 0
Driver Flags: Up Running Simplex
64BitSupport
Virtual Connections in use: 4
Max Virtual Connections in use: 5
Virtual Connections Overflow: 0
SVC UNI Version: uni3.1
IBM PCI 155 Mbps ATM Adapter Specific Statistics:
---------------------------------------------------
Total 4K byte Receive Buffers: 96 Using: 64
관련 정보
entstat 명령, fddistat 명령, netstat 명령, tokstat 명령.