| HOME / 정보공유 / AIX 명령어 모음

qosstat
qosstat qosstat 명령 목적 QoS(서비스의 품질 상태를 표시합니다. 구문
qosstat [ -A ] [ -n ] [ -a ]
설명
qosstat 명령은 설치된 Qos 정책에 대한 정보를 표시합니다.
파일
-A 각 정책에 대한 QoS 제어 블록의 주소를 표시합니다.
-n 네트워크 주소와 포트를 숫자로 표시합니다. 이 플래그없이, qosstat는 숫자 주소와 포트를 변환하고, 기호로 표시합니다.
-a 모든 정책을 표시합니다. 이 플래그없이, 연관된 연결이 있는 정책 조건만을 표시합니다.
예제
qosstat -na
Action:
Token bucket rate (B/sec): 10240
Token bucket depth (B): 1024
Peak rate (B/sec): 10240
Min policied unit (B): 20
Max packet size (B): 1452
Type: IS-CL
Flags: 0x00001001 (POLICE,SHAPE)
Statistics:
Compliant packets: 1423 (440538 bytes)
Conditions:
Source address Dest address Protocol
192.168.127.39:8000 192.168.256.29:35049 tcp (1 connection)
Action:
Token bucket rate (B/sec): 10240
Token bucket depth (B): 1024
Peak rate (B/sec): 10240
Outgoing TOS (compliant): 0xc0
Outgoing TOS (non-compliant): 0x00
Flags: 0x00001011 (POLICE,MARK)
Type: DS
Statistics:
Compliant packets: 335172 (20721355 bytes)
Non-compliant packets: 5629 (187719 bytes)
Conditions:
Source address Dest address Protocol
192.168.127.39:80 *:* tcp (1 connection)
192.168.127.40:80 *:* tcp (5 connections)